(module DGS0010A_N (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value DGS0010A_N (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 0) (layer F.SilkS))
  (fp_text user "*" (at 0 0) (layer F.Fab))
  (fp_text user ".Designator" (at -.125001 -1.2 270) (layer F.Fab))
  (fp_text user ".Designator" (at -.125001 -1.2 270) (layer Dwgs.User))
  (fp_text user "Designator9" (at -2.9972 -2.8448) (layer F.SilkS))
  (pad 1 smd oval (at -2.224999 -1.000001 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -2.224999 -.500002 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -2.224999 0 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -2.224999 .499999 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -2.224999 1.000001 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 2.225002 1.000001 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at 2.225002 .499999 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at 2.225002 0 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at 2.225002 -.500002 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 2.225002 -1.000001 90) (size .299999 1.35) (layers F.Cu F.Paste F.Mask))
)
