(module IC3_AP2138N-3.3TRG1_DIO (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IC3_AP2138N-3.3TRG1_DIO (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 0) (layer F.SilkS))
  (fp_text user "*" (at 0 0) (layer F.Fab))
  (fp_text user "0.022in/0.559mm" (at 0 -3.2766) (layer Cmts.User))
  (fp_text user "0.052in/1.321mm" (at 3.3274 1.1938) (layer Cmts.User))
  (pad 1 smd rect (at -.9525 1.1938) (size .5588 1.3208) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at .9525 1.1938) (size .5588 1.3208) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 -1.1938) (size .5588 1.3208) (layers F.Cu F.Paste F.Mask))
)
